This instruction is about to upgrade both sDP-1000EX's Main firmware and Audio USB module firmware.

The both firmware upgrade should be done at once.

How to upgrade the Main Firmware of sDP-1000EX

Preparations

Download sDP-1000EX's Main firmware.

sDP-1000Ex_V2.0a_20190607.hex

Download and install Flip software for the firmware upgrade.

Flip 3.4.7 software

Connect to sDP-1000EX

Connect sDP-1000EX to PC by a USB cable. Change the position of the red switch on the rear panel of sDP-1000EX to the DFU side. The red switch is next to Audio USB port. Turn on sDP-1000EX. The OLED won't display anything.

If, the OLED displays something, check the red switch's position, and then try to turn on the device again.

Run Flip program

Run Flip program.

Select a device

Click the button to select a device, and select AT90USB1286.

Connect the device

Select USB Port Connection and click Open button to be connected.

Select Firmware file

Select Load Hex File mene , and then select the download firmware.

Update Firmware

Click 'Run' button to update the firmware.

Finish upgrading the main firmware

업데이트가 완료되면, 전원을 끄고 sDP-1000EX 뒷면 Audio USB 포트 옆에 있는 빨간색 스위치를 다시 Audio로 변경하고 전원을 켭니다 Once the main firmware upgrade is finished, .

정상적으로 Audio 모드로 변경되었다면, 전면 OLED가 정상적으로 켜집니다.

만약, 전면 OLED이 켜지지 않는다면, 스위치를 다시한번 확인하시고 전원을 켜시기 바랍니다.

Audio USB 펌웨어 업그레이드 하기

준비

아래의 링크에서 Audio USB 펌웨어를 다운로드 합니다.

sDP-1000EX_USB_V6.C1_20190604.bin

SOtM 전용 드라이버가 설치되어 있지 않은 상태이면, 다음의 링크에서 드라이버를 다운 받아 설치 합니다.

SOtM USB Audio 2.0 Driver v2.23.0

SOtM USB Audio Firmware Upgrade 실행

sDP-1000EX을 PC와 USB 케이블로 연결한 후 sDP-1000EX의 전원을 켭니다.

SOtM USB Audio Firmware Upgrade 프로그램이 실행합니다.

펌웨어 파일 선택하기

'Browse 버튼을 클릭하고, 다운로드 한 펌웨어를 선택합니다.

펌웨어 업데이트 하기

'Start' 버튼을 클릭하여 펌웨어를 업데이트 합니다.

마무리하기

업데이트가 완료되면, SOtM USB Audio Control Panel을 실행하여 sDP-1000EX의 펌웨어 버젼을 확인합니다.

다운로드

==== sDP-1000EX FW 파일 ====a

sDP-1000Ex_V2.0a_20190607.hex

sDP-1000EX_USB_V6.C1_20190604.bin

유틸리티

Flip 3.4.7 software

SOtM USB Audio 2.0 Driver v2.23.0