sMS-1000SQ

sMS-1000SQ is a music file player and server, it browses, shares and plays music files in the network or stored in the product.

Windows Edition description

Eunhasu Edition description

Eunhasu usage

Exterior

Front Panel

Standby button: Power ON/OFF the unit.

Eject button: Eject an optical disk. (Use when an optional optical drive installed)

Indicator lamp: Indicate the power status. If the storage devices is operating, the lamp is blinking.

Rear Panel - sMS-1000SQu

Power input jack: Connect to a power supply.

Power input switch: Turn ON/OFF power of the unit.

Earth terminal: Connect to earth(ground).

External power input jack for AUDIO USB PORT: If you want to use external power to AUDIO USB PORT, you can use 6.5Vdc ~ 9Vdc, 2A power.

Power switch for AUDIO USB PORT: Turn ON/OFF +5.0v power of AUDIO USB PORT. If the connected USB audio device use USB port power, switch to ON.

AUDIO USB PORT: Connect to USB audio device.

USB port: Connect to non-USB audio device if needed.

LAN port: Connect to a router by network cable.

VGA port: Connect to a monitor by VGA cable if VGA display is needed.

HDMI port: Connect to a monitor by HDMI cable if HDMI display is needed.

Line-out jack: Main board analog audio output jack.

Mic-in jack: Main board microphone input jack.

Rear Panel - sMS-1000SQd

AES/EBU digital output: Connect to AES/EBU input of DAC.

Optical digital output: Connect to optical input of DAC.

Coaxial digital output: Connect to coaxial input of DAC.

Rear Panel - sMS-1000SQa

Right balanced analog audio output: Connect to right balanced analog audio input of amplifier.

Left balanced analog audio output: Connect to left balanced analog audio input of amplifier.

Right unbalanced analog audio output: Connect to right unbalanced analog audio input of amplifier.

Left unbalanced analog audio output: Connect to left balanced analog audio input of amplifier.