Squeezelite / Logitech Media Server

Squeezelite is a network music player which could be used with Logitech Media Server(aka. LMS). Eunhasu has LMS inside of itself which is available Tidal, Qobuz and internet radio.

Name: A name of device Squeezelite appearing on LMS. This could be changed if you need.

Audio device config: Select a radio button of USB DAC which is going to use and click ‘Save changes’ to use the USB DAC.

DSD mode: Set playback mode. Convert music to PCM or playing DSD music file by DoP or native. DAC should support native DSD when native mode.

Clear artwork.db: Delete LMS artwork database file. You should rescan in LMS to generate deleted file.

Clear config cache: Delete LMS config cache files.

LMS library rescan guide.

Move on to Settings menu page.

Click “Rescan” button to start scan on Basic Settings tab.

Click “Scanning - View Progress” link at bottom of page if you'd like to see scanning states.

Scanning states screen.

ickStream plugin provides lots of third-party feature like Quboz, TIDAL. Install guide are following.

http://wiki.ickstream.com/index.php/Open_Beta_Squeezebox_Installation

After finish ickStream plugin installation, you have to agree EULA and login ickStream in LMS > Settings > Advanced > ickStream page.

Login complete.

You can see ickStream item in My Apps of LMS main screen.

Video: how to install and set Spotify plugin in LMS; Spotify premium account required.